Author: Pat McMahon

“What each
Button does”
Pat’s Infrared Remote M

Pat McMahon Version 1 – 29/8/2018

Using Arduino, SONY Protocol
- Hexa Decimal Codes

Note– 40 possible active buttons.

0xA90 Power

0x290 Mute

0xB38 Audio
0x338 Picture
0x1EE9 Sound
0x6D0 Sleep
0x2CE9 AV Mode
0x6CE9 Input

0x738 Time
0x F38 System
0xCE9 Wide
0x5EE9 PC/
0x4CE9 Freeze
0x1CE9 Rotate

0x70 Menu

No Infra command

0x6D25 Exit
Infra= 16

0xA70 Daewoo
Infra= 16

0x2F0 Chinese TV
Infra= 72

0x2D0 JVC
Infra= 72

0xCD0 Thomson
Infra= 16

0xAF0 Prima
Infra= 16

0xE90 Surround
Infra= 72

0x37EE Return
Infra= 16

0x490 Vol +
Infra= 72

0xC90 Vol -
Infra= 72

0x10 Sharp 1
Infra= 72

0xC10 Sanyo 4
Infra= 72

0x610 Phillips 7
Infra= 72

0xB90 Hisense-/--
Infra= 72

Pat’s Infrared
Serial Monitor
Debug Program

Infrared Remote –M
To set to SONY Protocol
Power + 2 (SONY)

o

I

0xA50 TV/AV
Infra= 16

0x90 CH +
Infra= 16

0x5D0 Display
Infra= 16

0x890 CH -
Infra= 16

0x810 SONY 2
Infra= 16

0x410 Panasonic 3
Infra= 16

0x210 Hitachi 5
Infra= 16

0xA10 Toshiba 6
Infra= 16

0xE10 LG 8
Infra= 16

0x110 Samsung 9
Infra= 16

0x910 Skyworth 0
Infra= 16

0xDD0 Changhong
Infra= 16

LR-LCD-708E