/\*

\* Pat McMahon 23/7/2018 from basics.

\* A013-5x5 LED Matrix

\* LED's light up one at a time & stay on.

\* www.introtoarduino.com

\*

\*/

const int kPinLed1 = 2;

const int kPinLed2 = 3;

const int kPinLed3 = 4;

const int kPinLed4 = 5;

const int kPinLed5 = 6;

const int kPinLed6 = 7;

const int kPinLed7 = 8;

const int kPinLed8 = 9;

const int kPinLed9 = 10;

const int kPinLed10 = 11;

int delayTime=1000;

void setup()

{

pinMode(kPinLed1, OUTPUT);

pinMode(kPinLed2, OUTPUT);

pinMode(kPinLed3, OUTPUT);

pinMode(kPinLed4, OUTPUT);

pinMode(kPinLed5, OUTPUT);

pinMode(kPinLed6, OUTPUT);

pinMode(kPinLed7, OUTPUT);

pinMode(kPinLed8, OUTPUT);

pinMode(kPinLed9, OUTPUT);

pinMode(kPinLed10, OUTPUT);

}

void loop()

{

// turn on each of the LEDs in order

digitalWrite(kPinLed1, HIGH);

digitalWrite(kPinLed6, LOW);

delay(delayTime);

digitalWrite(kPinLed1, HIGH);

digitalWrite(kPinLed7, LOW);

delay(delayTime);

digitalWrite(kPinLed1, HIGH);

digitalWrite(kPinLed8, LOW);

delay(delayTime);

digitalWrite(kPinLed1, HIGH);

digitalWrite(kPinLed9, LOW);

delay(delayTime);

digitalWrite(kPinLed1, HIGH);

digitalWrite(kPinLed10, LOW);

delay(delayTime);

digitalWrite(kPinLed1, LOW);

digitalWrite(kPinLed2, HIGH);

digitalWrite(kPinLed6, LOW);

delay(delayTime);

digitalWrite(kPinLed2, HIGH);

digitalWrite(kPinLed7, LOW);

delay(delayTime);

digitalWrite(kPinLed2, HIGH);

digitalWrite(kPinLed8, LOW);

delay(delayTime);

digitalWrite(kPinLed2, HIGH);

digitalWrite(kPinLed9, LOW);

delay(delayTime);

digitalWrite(kPinLed2, HIGH);

digitalWrite(kPinLed10, LOW);

delay(delayTime);

digitalWrite(kPinLed2, LOW);

digitalWrite(kPinLed3, HIGH);

digitalWrite(kPinLed6, LOW);

delay(delayTime);

digitalWrite(kPinLed3, HIGH);

digitalWrite(kPinLed7, LOW);

delay(delayTime);

digitalWrite(kPinLed3, HIGH);

digitalWrite(kPinLed8, LOW);

delay(delayTime);

digitalWrite(kPinLed3, HIGH);

digitalWrite(kPinLed9, LOW);

delay(delayTime);

digitalWrite(kPinLed3, HIGH);

digitalWrite(kPinLed10, LOW);

delay(delayTime);

digitalWrite(kPinLed3, LOW);

digitalWrite(kPinLed4, HIGH);

digitalWrite(kPinLed6, LOW);

delay(delayTime);

digitalWrite(kPinLed4, HIGH);

digitalWrite(kPinLed7, LOW);

delay(delayTime);

digitalWrite(kPinLed4, HIGH);

digitalWrite(kPinLed8, LOW);

delay(delayTime);

digitalWrite(kPinLed4, HIGH);

digitalWrite(kPinLed9, LOW);

delay(delayTime);

digitalWrite(kPinLed4, HIGH);

digitalWrite(kPinLed10, LOW);

delay(delayTime);

digitalWrite(kPinLed4, LOW);

digitalWrite(kPinLed5, HIGH);

digitalWrite(kPinLed6, LOW);

delay(delayTime);

digitalWrite(kPinLed5, HIGH);

digitalWrite(kPinLed7, LOW);

delay(delayTime);

digitalWrite(kPinLed5, HIGH);

digitalWrite(kPinLed8, LOW);

delay(delayTime);

digitalWrite(kPinLed5, HIGH);

digitalWrite(kPinLed9, LOW);

delay(delayTime);

digitalWrite(kPinLed5, HIGH);

digitalWrite(kPinLed10, LOW);

delay(delayTime);

digitalWrite(kPinLed5, LOW);

// turn off each of the LEDs in order

}