`Bouncing Ball - On up button, Off Centre

`Pat McMahon-13/7/2019

`Motor connected to pin 1.

main:

infrain2 'wait for new signal from hand controller

if infra=**116** then Forwards 'Remote M-Up(116)switches on Motor High 1

if infra=**101** then AllOff 'Remote M-Up(116)switches on Motor High 1

goto main

Forwards: high **1**

goto main

AllOff: low **1**

goto main